incdir "tests"
include "dsp_base.inc"

;  Right here we are at a specific predetermined state.
;  Ideal environment to try instructions.
        
;  We can call send_back at any time to send data back to the PowerPC.

test_main:
  lri $AC0.M, #0x1000
  call send_back

  set40
  lri $AC0.M, #0x1000
  set16
  call send_back

; We're done, DO NOT DELETE THIS LINE
  jmp end_of_test
